1. Introduction  
2. Implementation and Benchmarking  
2.1 Tied-Array Beamforming with the MWA  
2.2 Multi-Pixel Beamforming Functionality  
2.3 Benchmarking  
3. Applications  
3.1 Testing the Validity of Calibration Solutions and Ionospheric Corrections  
3.2 Detection of Known Pulsars within a Field-of-View  
4. Discussion  
4.1 Survey Feasibility  
4.2 Implications for MWA Phase III and SKA-Low  
5. Summary